**German Financial Cooperation with the „Western Balkan Six Chamber Investment Forum” (WB6-CIF)**

**Regional Challenge Fund Project**

Procurement of IT equipment

Europe (non-EU), Montenegro (MNE)

Reference number: RCF/MNE/200059/G/2024/002

The answers to requests for clarifications received by the potential bidders to the following e-mail address: [procurement@rcf-wb6.org](mailto:procurement@rcf-wb6.org)

|  |  |
| --- | --- |
| **Q1** | Please correct the documentation in question, which concerns the conditions for participation in the procedure in question, because it is limiting for competition in the sense that only a certain number of bidders can submit a correct offer:  Manufacturer's Authorization  Manufacturer's Aftersales Declaration  Bearing in mind the above, we suggest that you remove the request for authorization so that more manufacturers can come into consideration, of course if you want to receive an offer from more bidders who can deliver and service this equipment.? |
| **A1** | **The mentioned documentation is required only for major items and in the case of NO bids with listed documentation is submitted, the Evaluation Committee may consider the submitted bids as acceptable.** |
| **Q2** | Interactive LED display - Includes accessory: card wireless  Interactive displays have integrated Wi-Fi as well as an antenna for amplifying the signal, so please explain to us why it is necessary to deliver a wireless card with the display. |
| **A2** | **Supplier doesn't have to deliver it as a separate accessory, if Wi-Fi is integrated.** |
| **Q3** | Interactive LED display:  Regarding the mobile stand, do you have any additional requirements such as height adjustment or similar? |
| **A3** | **More specifications:**  **Floor mobile mount type**  **Metallic/steel material**  **Can support screen size of Interactive LED display offered**  **Minimum load of 100kg**  **With detachable VESA plate**  **With 4 wheels for easy movement**  **Height adjustment capability is optional**  **Color black with powder coating surface is preferred.** |