**German Financial Cooperation with the „Western Balkan Six Chamber Investment Forum” (WB6-CIF)**

**Regional Challenge Fund Project**

Supply Tender „Procurement of technical equipment for cooperative training (CT) programme implementation “

 Europe (non-EU), North Macedonia (MKD)

Reference number: RCF/MKD/G/2023/001

The answers to requests for clarifications received by the potential bidders to the following e-mail address: procurement@rcf-wb6.org

|  |  |
| --- | --- |
| **Q1** | In file Annex 1. Technical Specifications - RCFMKDG2023001, Question refers to LOT No. 7 Workstations. Under item number 1.10 Aluminium Profile plate, required are four (4) pieces. According to the number Tables under point 1.8. Mobile worktable for Learntop-S and point 1.9. Learntop-A, our recommendation would be, that you require 12 Alu profileplates.Please advise, whether our proposal would be acceptable or increase the quantity at least to 8, otherwise some Learntops would be without profile plate. |
| **A1** | The proposal to increase the number of Aluminium Profile plates from four (4) pieces to eight (8) pieces is acceptable.*(Note : This change will be reflected in the Corrigendum No.1)* |
| **Q2** | In file Annex 1. Technical Specifications - RCFMKDG2023001, Question refers to Lot No.: 4 HYDRAULIC EQUIPMENT SETS. Under item number 4.7. Equipment set for Measurement and control in Hydraulics, there is a general requirement as follows:The set should be able to carry out the measurement experiments for proportional technology with recording characteristic curves and applications such as pressure stages and rapid traverse feed circuits, as well as control technology with position, sequence and pressure control. Sensors (e.g. pressure, flow and position) to be connected to the inputs and control signals to be transmitted to the EasyPort USB outputs. System requirements: PC with Windows XP10; Pentium III or equivalently; 2 GB RAM; CD-ROM disk drive; USB 2.0 or serial interface.We have a complete set available, but for the exercises for proportional and control hydraulics following components are also required:- Proportional amplifier - Displacement encoder for cylinder, 200 mm stroke - Mounting kit for cylinders - 4/3-way proportional valve - Proportional pressure relief valve - Pressure filter Adding listed components would influence the bid price. Please advise, whether our proposal would be acceptable to add additionally components mentioned before. |
| **A2** | It is not necessary to add additional components as long as the components required for the exercises on proportional and control hydraulics are components that are included in Lot 4 and in particular are among the main components in point 4.1 (basic proportional equipment set for hydraulic training) and point 2.1 (equipment set for basic training in control hydraulics). |