**German Financial Cooperation with the „Western Balkan Six Chamber Investment Forum” (WB6-CIF)**

**Regional Challenge Fund Project**

**CORRIGENDUM No.1**

**TO THE TENDER DOSSIER**

**Tender Dossier Title:** Procurement of technical equipment for cooperative training (CT) programme implementation

Europe (non-EU), North Macedonia (MKD)

**Tender Dossier Reference Number:** RCF/MKD/G/2023/001

**1. Reason for change**

Modification of requests provided in the technical specifications.

**2. Text to be corrected in the original tender dossier**

Annex 1. Technical Specifications, Lot No.: 7 WORKSTATIONS

Instead of:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Budget item name and number** | **Quantity** | **Unit** | **Specifications required** | **Technical Specifications Offered** | **Notes, remarks, ref to documentation** | **Evaluation Committee’s notes** |
| **1. Mobile laboratory workbench** | 1 | set |  |  |  |  |
| 1.1. Mobile laboratory workbench | 1 | piece | Mobile laboratory workbench should be suitable for hydraulic, pneumatic and electrotechnical training; must offer unlimited range of configuration possibilities for the Learnline workstation; Individual and group training workstations; possibility to be transported through doors; allow two different groups to train simultaneously on both sides. Double pump power unit and up to two compressors to fit easily on the frame. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.2. Fixed drawer unit for installation in Mobile laboratory workbench with 4 drawers. | 1 | piece | Fixed drawer unit with 4 drawers for pneumatic equipment sets. Drawer unit with fully extending lockable steel drawers with safety stop. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.3. Fixed drawer unit for installation in Mobile laboratory workbench with 3 drawers. | 1 | piece | Fixed drawer unit with 3 drawers for hydraulic equipment sets. Drawer unit with fully extending lockable steel drawers with safety stop. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.4. Storage plate for the basic mobile unit | 1 | piece | To be fitted into the mobile frame in addition to 2 drawer units and to offer installation space for 2 air compressors. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.5. Universal bracket for hydraulic | 1 | piece | To be able to give the ability to mount quick couplers; to allow to easily connect and disconnect various implements; to permits the mounting of up to 2 hydraulic power units with single pump, up to 2 hydraulic measuring containers or holders for storing hoses. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.6. Holder for up to 20 hydraulic hoses | 1 | piece | Able to hold up to 20 hydraulic hoses; to provide neat storage and to protects hose couplings from ingress of dirt. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.7. Holder for laboratory cables | 1 | piece | Portable cable holders to store laboratory cables and to ensure that cables are kept neatly and in order. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.8. Mobile worktable for Learntop-S | 4 | piece | To be used on the workstation for hydraulic training; drawer unit with 8 fully extending drawers; storage space with lockable sliding doors; steel tub tabletop. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.9. Learntop-A | 4 | piece | Lerntop to be used on one side of the workstation for pneumatic and electrotechnical training and suitable to hold up different profile plates ((to 2 profile plates of size up to 350 x 1100 mm or one profile plate of size up to 700 x 1100 mm). | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.10. Aluminium-Profilplatte | 4 | piece | The components of the anodized aluminum profile plate to be fitted securely and safely into the grooves on the profile plate; both sides to be fitted with components; the grooves to be compatible with the ITEM profile system. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |

Read:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Budget item name and number** | **Quantity** | **Unit** | **Specifications required** | **Technical Specifications Offered** | **Notes, remarks, ref to documentation** | **Evaluation Committee’s notes** |
| **1. Mobile laboratory workbench** | 1 | set |  |  |  |  |
| 1.1. Mobile laboratory workbench | 1 | piece | Mobile laboratory workbench should be suitable for hydraulic, pneumatic and electrotechnical training; must offer unlimited range of configuration possibilities for the Learnline workstation; Individual and group training workstations; possibility to be transported through doors; allow two different groups to train simultaneously on both sides. Double pump power unit and up to two compressors to fit easily on the frame. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.2. Fixed drawer unit for installation in Mobile laboratory workbench with 4 drawers. | 1 | piece | Fixed drawer unit with 4 drawers for pneumatic equipment sets. Drawer unit with fully extending lockable steel drawers with safety stop. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.3. Fixed drawer unit for installation in Mobile laboratory workbench with 3 drawers. | 1 | piece | Fixed drawer unit with 3 drawers for hydraulic equipment sets. Drawer unit with fully extending lockable steel drawers with safety stop. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.4. Storage plate for the basic mobile unit | 1 | piece | To be fitted into the mobile frame in addition to 2 drawer units and to offer installation space for 2 air compressors. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.5. Universal bracket for hydraulic | 1 | piece | To be able to give the ability to mount quick couplers; to allow to easily connect and disconnect various implements; to permits the mounting of up to 2 hydraulic power units with single pump, up to 2 hydraulic measuring containers or holders for storing hoses. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.6. Holder for up to 20 hydraulic hoses | 1 | piece | Able to hold up to 20 hydraulic hoses; to provide neat storage and to protects hose couplings from ingress of dirt. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.7. Holder for laboratory cables | 1 | piece | Portable cable holders to store laboratory cables and to ensure that cables are kept neatly and in order. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.8. Mobile worktable for Learntop-S | 4 | piece | To be used on the workstation for hydraulic training; drawer unit with 8 fully extending drawers; storage space with lockable sliding doors; steel tub tabletop. | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| 1.9. Learntop-A | 4 | piece | Lerntop to be used on one side of the workstation for pneumatic and electrotechnical training and suitable to hold up different profile plates ((to 2 profile plates of size up to 350 x 1100 mm or one profile plate of size up to 700 x 1100 mm). | [Manufacturer/Brand] [Model] [Offered specifications] |  |  |
| **1.10. Aluminium-Profilplatte** | **8** | **piece** | **The components of the anodized aluminum profile plate to be fitted securely and safely into the grooves on the profile plate; both sides to be fitted with components; the grooves to be compatible with the ITEM profile system.** | **[Manufacturer/Brand] [Model] [Offered specifications]** |  |  |

All other terms and conditions of the tender dossier remain unchanged. The above corrections to the tender dossier are integral part of the tender dossier.